COMPOSTING TOILET

The Nature’s Head Composting toilet is the most innovative design, offers the best value and the most reliable solution for personal sanitation requirements of any product in the field.

The toilet is self-contained, urine diverting and the waterless operation allows for ease of use for many applications. The Nature’s Head is lightweight, odorless and compact making it a perfect fit for your home, cabin, tiny house, RV, workshop, boat and survival application.

The toilet with its stainless steel hardware, robust construction and user friendliness has been designed to withstand the harshest of conditions.

We take great pride in offering a product which we manufacture in the United States and strive to provide exceptional customer service.

[image: image1.jpg]Comfortable, Safe, Easy

» Elongated molded seat
eEasy Cleaning
eComfortable
esafe

» Urine Separating
*Even when trap door is open
eMales may either sit or stand

» After Use
eAgitator crankis turned a
couple of times



[image: image2.png]Economic Advantages

«Reduced water consumption;
no water required for flushing

«Eco-friendly
Works in any temperature

oEasily installed; low
installation cost -

 Elimination of need to find
and travel to pump-out facil

Most competitively priced
self-contained toilet




[image: image3.png]Innovative Design

» Molded Seat

*Easy toclean
*Durable
Never needs replacement

» Urine Separating
#No Odor
<High Capacity
*Easy to empty

»Rugged
*Polyethylene
Al marine grade stainless.
teel fittings
directional agitator handles




[image: image4.png]Compact
Design

®Entirely Self-Contained

®Baseis 127 "tall

eOverall length is 17 3"

eTotal Height is less
than 21%"

®Seat Height is 20"
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. Narrow Spaces

The base is only 13" wide at
the bottom.

e e Overall Width:
iﬁ Standard Handle =20 % "
swsndus. SPider Handle =17 3/4”




[image: image6.png]Choice of Agitator Handles

Two agitator handle configurations are available. Both
systems provide for bi-directional cranking. Spider handle
reduces the overall width of the unit by 2 %”. Handles can
be mounted on either side.

STANDARD AGITATOR



[image: image7.png]Space Requirements

If the unit is mounted
against a wall, allow 2"
for the top to pivot for
removal of the bottle
and the top.




[image: image8.png]Easy Installation

o5 feet of venting hose with ends

einside vent flange

«agitator handle

2mounting brackets and knobs

« 6 feet wiring for internal fan
hook-up required for 12V system

ofuse holder and fuse for direct
battery attachment

eliquids tank cap

eInstruction Booklet

Also included:
*4 mounting bolts (for wood floor installations)
« Allen wrench for installation spider handle



[image: image9.png]Brackets and Crank Installed




[image: image10.png]Easy Installation

The unit attaches to the floor

with two small L-brackets. e
There is one ventilation hose to

run outside and one 12volt

power hook-up for a small

computer type fan. Can also be
run using our 110 volt adapter.

Powerless operation can be installed

by using a solar vent ﬂ
N
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The electric receptacle
for the 12Voltor 110
adaper is conveniently
located on the top right
ofthe fan housing.

The vent hose s
attached to the fan side.




[image: image12.png]Filter and Fan Housing

The filter and the fan
housing can be
switched to either
side.

The opposite housing
contains the filter.




[image: image13.png]Emptying the Liquids

The urine bottle holds 2.2
gallons.

To empty,simply lip the
twolatches on the sides
andft the upper section
up a few inches. Put the lid
on the liquid bottle and lft
itout ofits holder.




[image: image14.png]The Solids Bin

‘The Solids Bin will accommodate 60-80 uses depending
on the composting time.

Approximately 2 gallons of peat moss is used, tofill to
the level of the agitator in a horizontal position. Peat
moss is moistened with water before adding.




[image: image15.png]Removing the Unit Top

The top pivots, and is held in place by a stainless
steel slip hinge. It is removed by simply sliding
the top of the unit 2" to the left to disengage.




[image: image16.png]Emptying the Solids

Aregular kitchen trash
bag fits the base. Just
invert. After dumping,
add new peat moss.

Noneed to clean as any-
thing left helps to restart
the composting process.



[image: image17.png]Optional Lid for Solids Bin

An optional vented
lidis available if you
prefer to carry the
base to a disposal
faclity.




[image: image18.png]Extended Capacity

Extra bases, com-
plete with lids, for
storage allow for
further composting
and extend the use.
of the unit.




[image: image19.png]Extra Bottles Available

Extra bottles, with
caps, are available for
‘when additional
capacity is needed.




[image: image20.png]Five Year Warranty

Nature's Head
carties a full 5-Year
warranty.

We pride ourselves
on our excellent
customer service
record.




[image: image21.png]Safely Shipped

Twolocking inserts, designed especially for the
Nature's Head Composting Toilet insure against
damage during shipping, while minimizing
shipping weight and waste. Inserts and shipping
boxes are all recyclable.




[image: image22.png]*Homes
*Boats

RVS

«Cabins

oSheds

*0ff-Grid Residences
*Bams

«Pool Change rooms
«Cottages

*Garages

*Work Shops

*Boat Houses

Anywhere a Toilet is Needed!





What sets us apart!

· Proudly made in the USA.

· Five Year Warranty

· All stainless hardware.

· Full size elongated seat for comfort.

· Disassembles in seconds for emptying.

· Composting handle can be mounted on either side.

· Vent hose and fan may be mounted on either side.

· Unit comes with everything for your installation but the external vent.

· Molded in toilet seat for safety and ease of cleaning.

· Completely self contained and portable.

· Fully supported liquid tank for applications where it extends beyond mounting pedestal

· Translucent liquid tank allows for easy visual capacity inspection.

· Rear of main tank is angled for hull-side installation on boats..

· It's AFFORDABLE!

